
                 ---------------------------------   
              	       -- CA TRANSFER V3.1 --
                 ---------------------------------
                 
 --------------
  Requirements
 --------------

 IBM PC or compatible (Pentium or better)
 Microsoft(R) Windows(R) 98 / NT 4 / 2000 / Me / XP / Vista



 ---------
  Install
 ---------

 Run SETUP.EXE



 ---------
  Warning
 ---------

 The communication baudrate should be 19200 baud for the RS232 PC interface
with no parity , Data 8 bit and 1 Stop bit.

 After the Install, the option "Save settings on exit" 
and the language "English" are notched by default.

 The CA Transfer software operates perfectly with Windows Vista,
except that the help files can only be displayed after installing 
a Microsoft patch which is available for download.
A corrective measure of Microsoft which can be downloaded
with following address Internet: 
http://www.programmez.com/telechargements.php?id_logiciel=187

 ---------
  Data
 ---------

 Two types of files are managed by CA TRANSFER V3.1
	
	- A type of file with extension *.dat 
	which contains the data sent by the F27 in scan transmission mode with a scan value different from 0.

	- A type of file with extension *.trf
	which contains the data sent by the F27 in single transmission mode with a scan value equal to 0.
